# **Usage:**

Medium demolition. It can break thick concrete, boulders, stone, frozen ground, etc… It can also drive pickets, ground rods, pipes and railroad spikes.

# **Specifications:**

* Tooling size: 1 1/8” Hex Tooling
* Blows/Min: 860
* Single impact energy 50.2lbs
* Weight: 65lbs

# **Safety:**

* Must use eye protection.
* Use proper lifting technique.
* Be aware of surroundings.
* Never handle breaker tooling without gloves because of the burn danger

# **operations**

* Select correct tooling; moil point, chisel, and pavement cutter.
* Confirm that tooling is securely attached to breaker.
* Always hold the breaker down firmly on the work surface before depressing the throttle.
* Avoid embedding breaker tooling.

# **maintenance:**

* Wipe down breaker and tooling with WD40 prior to storage

