# **Usage:**

Capable of reducing the lifting/pulling line force by 75%.

# **Specifications:**

* Hardware: 11,800 lbs MBS
* Rope: 10,341lbs MBS @ 150’

# **operation:**

**Application**

* Piggy back on existing line with prussic loop
* Pull in-line with system
* Disengage gain-saver cam while stretching pulleys to length
* Use gain-saver cam while hauling

# **key points:**

* Apply directly to anchor and load, or piggyback on existing line w/ prussic loop.
* Pull in-line with system
* Disengage gain-saver cam while stretching pulleys to length
* Use gain-saver cam while hauling

# **maintenance:**

* ****Clean and inspect after each use