# **Usage:**

Provides hard-line duplex communications for up to four personnel. The unit has a hard-line intercom, is self-powered and portable.

# **Specifications:**

* CSI-2100 unit Powered by: 3 “C” size batteries
* CSI-2140 Alarm Module Powered by: 4 “C” size batteries
* Kit includes a Double Splitter, a Single Splitter and a “Talk Box”

# **Safety:**

**Test before putting system into an “IDLH” atmosphere. Do not change batteries in IDLH atmosphere**

* Do not put tension on cables
* Check low battery indicator before putting into use.

# **operations:**

* Remove all components from carrying case
* Connect CSI- 2100 Command module to the Alarm Module via cable
* Connect Operator’s Headset
* Connect appropriate Splitter if necessary
* Connect Talk Box if necessary
* Connect orange comm. lines to Entrants Throat Mic/Face Mask Speaker
* Turn Command Module on and set volumes
* Test Alarm Module
* Test Comm. system with Entrants

# **Maintenance:**

* Replace batteries as needed. (Refer to the owner’s manual section 3)
* System is waterproof and can be cleaned and washed off if necessary
* Contaminated cables jackets should be cleaned with Mineral Spirits (Connect ends before cleaning)
* Use dust covers on unused sockets
* Do not put strong tension on cables. Use cable strain relief snap hooks