# **Usage:**

The Partner K950 Rescue saw can be used for various cutting applications from steel to masonry.

# **Specifications:**

**Partner K970**

* 2 stroke
* 94cc
* 6.1hp
* Weight: 23lbs.
* Maximum spindle speed: 9,800rpm
* Fuel Capacity: 2.65pts
* Carburetor: Tillotson HS 282A (K950) and Walbro RWJ-3A (K970)
* SmartCarb System: allows saw to always operate with the proper fuel to air mixture by linking the fuel chamber pressure to the filter intake chamber

# **fire department modifications**

* Chrome blade guard for better visibility
* Large D-grip starter handle
* Mounted Sling assembly, and LED light
* Decompression Button
* Reduces the force necessary to start the saw by 50%
* Active Air Filtration
* 3 Stage Filter
* Internal and fully sealed
* Equipped with Ready Start
* Allows user to stop the motor and pull start later without resetting anything

# **mk diamond tiger tooth blade:**

* Cuts steel, masonry, rebar, corrugated roofing, case hardened steel, Nader Bolts, Lexan, and window bars.
* Vacuum Brazed Technology
* Diamond particles are fused directly to the steel core

# **operations:**

* Place Saw on the ground
* Push the decompression button
* Lock the trigger
* Pull the choke out and pull the starter handle
* Once started push the choke back in
* To turn off, pull the stop button out

# **maintenance:**

* Allow to cool before topping off fuel
* Check for damage and check belt tension
* Wipe down and remove debris