# **Usage:**

Video Diagnostic tool used to search void/confined spaces.

# **Specifications:**

* 5” Color LCD Video Screen
* High Speed CCD color camera with built in LED lights
* Ring Adapter
* Camera articulates up to 135 degrees
* 2’ to 4’ extension pole

# **operations:**

* Connect camera to desired adapter. (18” Wand, 2’-4’ extension pole, or ring adapter)
* Connect appropriate monitor/camera head connector cable to adapter and monitor
* Depress power button (Center/Green)
* Manipulate selected adapter to view images
* Increase light intensity as needed (Red Button, three different settings)
* Rotate picture as necessary (Blue Button)

# **Maintenance:**

* Wipe clean all components after use
* Check all cords for damage
* Rotate batteries every Monday per schedule
* Check camera lens for damage
* Replace all components in the carrying case