# **Usage:**

Personal travel restrictor and mini MA.

# **Specifications:**

* Swivel “omni” pulleys (blocks) are hewn from a solid “block” of high strength aluminum and are engineered to withstand over 8,000# (36kN) of tensile force end to end.
* 8mm restraint cord, rated at 4,270# (19kN) and both ratchets in two colors, and shock absorber/restraint cords.

# **safety:**

**N/A**

# **operation:**

* Turn the set-of-fours one way and you have a 5:1 mechanical advantage, turn it around and a 4:1 w/change of direction.
* Other end is a personal travel restrictor.

# **maintenance:**

* Blocks should be inspected before and after use to insure that connecting hardware is intact.
* All software should be inspected for wear and glazing. These should be replaced as this occurs before use

