# **Usage:**

The Hurst Ram is used for quick access to locations where spreaders will not fit. Rams Give Much higher spread and lifting capabities

# **Specifications:**

* Piston Stroke: 14.2”
* Lifting Force 23,154 lbs
* Extended Length 35.6’’
* Extended length with EXT 47.2”

# **operations:**

* Turn ON/OFF switch
* Use Deadman switch to open and close cutter
* After use leave cutter slightly open
* Wipe down and inspect for damage

# **maintenance:**

* Remove dirt and debris by wiping down
* Use WD-40 to lubricate fittings

