# **Usage:**

The salvage covers are used to protect people’s belongings. We can also use salvage covers to catch and divert water, triage applications, and staging gear.

# **Specifications:**

**Treated Canvas Cover**

* 12’x18’
* Grommets
	+ Approximately 32” apart
	+ 5/8” diameter
	+ Brass to resist rust and corrosion
* Cotton Duck “Canvas”-
	+ Impregnated with wax
	+ Treated to resist water, mildew and rot
* Tightly woven
* Strong, durable and snag resistant
* Flame Retardant
* Fabric weight: 12 oz / sq yard before treatment and 18 oz / sq yard after treatment.

**Polyethylene**

* 12’x18’
* 6 oz per sq. yard
* 1000 Denier
	+ A very heavy weight nylon with a urethane coating
* Grommets
* Approximately 32” apart
* 5/8” diameter
* Brass to resist rust and corrosion

# **other Equipment:**

* S-hooks or nails
* 8” wide to fit the depth of the shelf

# **operations:**

* Pay out method
* Balloon Throw
* Accordion Throw
* Accordion Fold
* Clean and Dirty sides

# **maintenance:**

* Inspect for wear and abrasions
* Hold up to the sunlight to inspect for holes
* Sweep out air and let dry